DICOM PS3.18 2018e - Web Services

6.9.4.3.2 Response Message (Current)
Prev | 6.9.4.3 Response | Next

##### 6.9.4.3.2 Response Message

The response message body contains the results.

The format of the response message body shall contain one of the Media Types specified by the request Accept header field. An Origin-Server shall support all Media-Types allowed in the request.

###### 6.9.4.3.2.1 XML Response Message

- Content-Type:

  - application/dicom+xml

- The response contains a DICOM PS3.19 XML DicomNativeModel element containing the attributes for the requested UPS Instance (see Section A.1 in PS3.19 ).

###### 6.9.4.3.2.2 JSON Response Message

- Content-Type:

  - application/dicom+json

- The response is a DICOM JSON array containing a DICOM JSON representation of the requested UPS Instance (see Section F.2).

Prev | Up | Next
6.9.4.3 Response | Home | 6.9.5 ChangeUPSState

DICOM PS3.18 2018e - Web Services