DICOM PS3.16 2018e - Content Mapping Resource

TID 5026 OB-GYN Pelvic Vascular Ultrasound Measurement Group (Current)
Prev | OB-GYN Report Templates | Next

### TID 5026 OB-GYN Pelvic Vascular Ultrasound Measurement Group

This Template is an anatomy specific container of OB-GYN pelvic vascular measurements.

Table TID 5026. Parameters

Parameter Name | Parameter Usage
--- | ---
$AnatomyGroup | The concept name of the vascular anatomy

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 5026. OB-GYN Pelvic Vascular Ultrasound Measurement Group

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | $AnatomyGroup | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (G-C171, SRT, "Laterality") | 1 | MC | IFF anatomy has laterality | DCID 244 “Laterality”
3 | > | HAS CONCEPT MOD | TEXT | EV (112050, DCM, "Anatomic Identifier") | 1 | U |  |
4 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1-n | M |  | $MeasType = DCID 12119 “Vascular Ultrasound Property” $Derivation = DCID 3627 “Measurement Type”
5 | >> | HAS CONCEPT MOD | CODE | EV (125105, DCM, "Measurement Orientation") | 1 | U |  | DCID 12118 “Measurement Orientation”
6 | >> | HAS PROPERTIES | NUM | EV (125106, DCM, "Doppler Angle") | 1 | U |  | UNIT = EV (deg, UCUM, "deg")
7 | >> | HAS PROPERTIES | NUM | EV (125107, DCM, "Sample Volume Depth") | 1 | U |  | UNIT = EV (cm, UCUM, "cm")

Content Item Descriptions

Row 1 | Specifies the anatomical context of the observations in the group.
Row 3 | Differentiates between multiple structures such as the two umbilical arteries.

Prev | Up | Next
TID 5025 OB-GYN Fetal Vascular Ultrasound Measurement Group | Home | Vascular Ultrasound Report Templates

DICOM PS3.16 2018e - Content Mapping Resource