DICOM PS3.2 2018e - Conformance

D.4.2.3 STORAGE-SCU (Current)
Prev | D.4.2 AE Specifications | Next

#### D.4.2.3 STORAGE-SCU

##### D.4.2.3.1 SOP Classes

STORAGE-SCU provide Standard Conformance to the following SOP Class(es) :

Table D.4.2-12. SOP Classes Supported By STORAGE-SCU

SOP Class Name | SOP Class UID | SCU | SCP
--- | --- | --- | ---
Stored Print Storage | 1.2.840.10008.5.1.1.27 | Yes | No
Hardcopy Grayscale Image Storage | 1.2.840.10008.5.1.1.29 | Yes | No
Hardcopy Color Image Storage | 1.2.840.10008.5.1.1.30 | Yes | No
Computed Radiography Image Storage | 1.2.840.10008.5.1.4.1.1.1 | Yes | No
Digital X-Ray Image Storage - For Presentation | 1.2.840.10008.5.1.4.1.1.1.1 | Yes | No
Digital X-Ray Image Storage - For Processing | 1.2.840.10008.5.1.4.1.1.1.1.1 | Yes | No
Digital Mammography X-Ray Image Storage - For Presentation | 1.2.840.10008.5.1.4.1.1.1.2 | Yes | No
Digital Mammography X-Ray Image Storage - For Processing | 1.2.840.10008.5.1.4.1.1.1.2.1 | Yes | No
Digital Intra-oral X-Ray Image Storage - For Presentation | 1.2.840.10008.5.1.4.1.1.1.3 | Yes | No
Digital Intra-oral X-Ray Image Storage - For Processing | 1.2.840.10008.5.1.4.1.1.1.3.1 | Yes | No
CT Image Storage | 1.2.840.10008.5.1.4.1.1.2 | Yes | No
Ultrasound Multi-frame Image Storage (Retired) | 1.2.840.10008.5.1.4.1.1.3 | Yes | No
Ultrasound Multi-frame Image Storage | 1.2.840.10008.5.1.4.1.1.3.1 | Yes | No
MR Image Storage | 1.2.840.10008.5.1.4.1.1.4 | Yes | No
Enhanced MR Image Storage | 1.2.840.10008.5.1.4.1.1.4.1 | Yes | No
MR Spectroscopy Storage | 1.2.840.10008.5.1.4.1.1.4.2 | Yes | No
Standalone Modality LUT Storage | 1.2.840.10008.5.1.4.1.1.10 | Yes | No
Standalone VOI LUT Storage | 1.2.840.10008.5.1.4.1.1.11 | Yes | No
Grayscale Softcopy Presentation State Storage | 1.2.840.10008.5.1.4.1.1.11.1 | Yes | No
X-Ray Angiographic Image Storage | 1.2.840.10008.5.1.4.1.1.12.1 | Yes | No
X-Ray Radiofluoroscopic Image Storage | 1.2.840.10008.5.1.4.1.1.12.2 | Yes | No
X-Ray Angiographic Bi-Plane Image Storage (Retired) | 1.2.840.10008.5.1.4.1.1.12.3 | Yes | No
Nuclear Medicine Image Storage | 1.2.840.10008.5.1.4.1.1.20 | Yes | No
Raw Data Storage | 1.2.840.10008.5.1.4.1.1.66 | Yes | No
VL Image Storage (Retired) | 1.2.840.10008.5.1.4.1.1.77.1 | Yes | No
VL Multi-frame Image Storage (Retired) | 1.2.840.10008.5.1.4.1.1.77.2 | Yes | No
VL Endoscopic Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.1 | Yes | No
VL Microscopic Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.2 | Yes | No
VL Slide-Coordinates Microscopic Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.3 | Yes | No
VL Photographic Image Storage | 1.2.840.10008.5.1.4.1.1.77.1.4 | Yes | No
Basic Text SR | 1.2.840.10008.5.1.4.1.1.88.11 | Yes | No
Enhanced SR | 1.2.840.10008.5.1.4.1.1.88.22 | Yes | No
Comprehensive SR | 1.2.840.10008.5.1.4.1.1.88.33 | Yes | No
Mammography CAD SR | 1.2.840.10008.5.1.4.1.1.88.50 | Yes | No
Key Object Selection Document | 1.2.840.10008.5.1.4.1.1.88.59 | Yes | No
Positron Emission Tomography Image Storage | 1.2.840.10008.5.1.4.1.1.128 | Yes | No
Standalone PET Curve Storage | 1.2.840.10008.5.1.4.1.1.129 | Yes | No
RT Image Storage | 1.2.840.10008.5.1.4.1.1.481.1 | Yes | No
RT Dose Storage | 1.2.840.10008.5.1.4.1.1.481.2 | Yes | No
RT Structure Set Storage | 1.2.840.10008.5.1.4.1.1.481.3 | Yes | No
RT Beams Treatment Record Storage | 1.2.840.10008.5.1.4.1.1.481.4 | Yes | No
RT Plan Storage | 1.2.840.10008.5.1.4.1.1.481.5 | Yes | No
RT Brachy Treatment Record Storage | 1.2.840.10008.5.1.4.1.1.481.6 | Yes | No
RT Treatment Summary Record Storage | 1.2.840.10008.5.1.4.1.1.481.7 | Yes | No

Prev | Up | Next
D.4.2.2.4 Association Acceptance Policy | Home | D.4.2.3.2 Association Policies

DICOM PS3.2 2018e - Conformance