DICOM PS3.17 2018e - Explanatory Information

TTT.2.3.4 Example (Current)
Prev | TTT.2.3 Case #3: Reconstruction From A Sub-region of All Image Frames | Next

#### TTT.2.3.4 Example

In this example, the slices of the two volumes are reconstructed in the axial plane of the patient; the row direction is aligned in the positive x-direction of the patient (right-left) and the column direction is aligned in the positive y-direction of the patient (anterior-posterior).

The full field of view reconstruction in encoded with the Instance UID "Z1" and consists of a 512 cube volume of 0.2 mm of voxel size. The sub-region reconstruction in encoded with the Instance UID "Z2" and consists of a 256 cube volume of the voxel size of 0.1 mm.

Both volumes share the same Frame of Reference UID.

Figure TTT.2.3-2. Attributes of 3D Reconstruction of the full field of view of the projection frames

Figure TTT.2.3-3. Attributes of 3D Reconstruction using a sub-region of all frames

Prev | Up | Next
TTT.2.3.3 Encoding Details | Home | TTT.2.4 Case #4: Multiple Rotations, One Or More 2D Instances, One Reconstruction, One X-Ray 3D Instance

DICOM PS3.17 2018e - Explanatory Information