DICOM PS3.4 2018e - Service Class Specifications

GG.6.2.2 Display Application (Current)
Prev | GG.6.2 Color Palette Storage SOP Class | Next

#### GG.6.2.2 Display Application

An implementation that conforms to the Color Palette Storage SOP Class as an SCP and interprets the contents of instances of the SOP Class to affect the display of images, shall apply all mandatory Color Palette and presentation intent Attributes to the applicable displayed images.

An implementation that conforms to the Color Palette Storage SOP Class as an SCP and interprets the contents of instances of the SOP Class to affect the display of images shall state in its Conformance Statement:

- The optional Attributes of the Color Palette IOD that it is capable of interpreting and those that are not supported.

- The Image Storage SOP Classes for which application of the Color Palette Storage SOP Class is supported

Prev | Up | Next
GG.6.2 Color Palette Storage SOP Class | Home | GG.6.3 Template Storage SOP Classes

DICOM PS3.4 2018e - Service Class Specifications