DICOM PS3.16 2018e - Content Mapping Resource

TID 3216 Stenotic Flow Reserve (Current)
Prev | Quantitative Arterial Analysis Report SR IOD Templates | Next

### TID 3216 Stenotic Flow Reserve

The Stenotic Flow Reserve Template consists of a CONTAINER providing quantitative arterial analysis measurements derived for an obstruction in a total analyzed segment.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3216. Stenotic Flow Reserve

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (122548, DCM, "Stenotic Flow Reserve") $Unit = DT ({ratio}, UCUM, "ratio")
2 |  | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (122549, DCM, "Poiseuille Resistance") $Unit = DT (mm[Hg].s/cm, UCUM, "mmHG.s/cm")
3 |  | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (122550, DCM, "Turbulence Resistance") $Unit = DT (mm[Hg].s2/cm2, UCUM, "mmHG.s2/cm2")
4 |  | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (122555, DCM, "Estimated Normal Flow") $Unit = DT (ml/s, UCUM, "ml/s")
5 |  | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = EV (122551, DCM, "Pressure Drop at SFR") $Unit = DT (mm[Hg], UCUM, "mmHg")
6 |  | CONTAINS | IMAGE | No purpose of reference | 1 | U |  |

Content Item Descriptions

Row 6 | Secondary Capture image with SFR analysis contour

Prev | Up | Next
TID 3215 Angiographic Lesion Analysis | Home | TID 3217 Sub-segmental Data

DICOM PS3.16 2018e - Content Mapping Resource