DICOM PS3.3 2018e - Information Object Definitions

C.36.7 Intended RT Treatment Phase Module (Current)
Prev | C.36 RT Second Generation Modules | Next

### C.36.7 Intended RT Treatment Phase Module

RT Treatment Phases define the intended phases of treatment and their temporal relationship.

Table C.36.7-1. RT Treatment Phase Intent Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Intended RT Treatment Phase Sequence | (3010,004B) | 1 | RT Treatment Phase definitions. RT Treatment Phases define the relationships between RT Radiation Set Instances which contain the treatment parameters for the radiation to be concurrently and/or subsequently delivered. The RT Treatment Phase Index (3010,003A) shall define the temporal sequencing of the phases. One or more Items shall be included in this Sequence.
>Include Table C.36.2.1.2-1 “RT Treatment Phase Macro Attributes” | The RT Treatment Phase Index (3010,003A) shall start at 1 and increase monotonically by 1 for successive Items in this Sequence.
Include Table C.36.2.1.3-1 “RT Treatment Phase Interval Macro Attributes” |

Prev | Up | Next
C.36.6 RT Enhanced Prescription Module | Home | C.36.8 RT Segment Annotation Module

DICOM PS3.3 2018e - Information Object Definitions