DICOM PS3.3 2018e - Information Object Definitions

C.8.27.2.4 Bits Allocated, Bits Stored and Samples Per Pixel (Current)
Prev | C.8.27.2 Intravascular OCT Image Module | Next

##### C.8.27.2.4 Bits Allocated, Bits Stored and Samples Per Pixel

For IVOCT images, Bits Allocated (0028,0100), Bits Stored (0028,0101) Samples Per Pixel (0028,0002) are specified to use the following values for Presentation Intent Type (0008,0068) Attribute:

Table C.8.27.2-5. Bits Allocated/Stored

Presentation Intent Type | Bits Allocated / Bits Stored | Samples Per Pixel
--- | --- | ---
FOR PRESENTATION | 8/8, 16/12 or 16/16 | 1
FOR PROCESSING | 8/8, 16/12 or 16/16 | 1

Prev | Up | Next
C.8.27.2.3 Pixel Presentation | Home | C.8.27.3 Intravascular OCT Acquisition Parameters Module

DICOM PS3.3 2018e - Information Object Definitions