DICOM PS3.17 2018e - Explanatory Information

R.5 Shutdown (Current)
Prev | R Configuration Use Cases (Informative) | Next

## R.5 Shutdown

### R.5.1 Shutdown

The lease timeouts eventually release the IP address at DHCP, which can then update DNS to indicate that the host is down. Clients that utilize the hostname information in the LDAP database will initially experience reports of connection failure; and then after DNS is updated, they will get errors indicating the device is down when they attempt to use it. Clients that use the IP entry directly will experience reports of connection failure.

Prev | Up | Next
R.4 Device Start up | Home | R.5.2 Online/offline

DICOM PS3.17 2018e - Explanatory Information