DICOM PS3.2 2018e - Conformance

E.8.5 Standard Extended / Specialized / Private SOP Classes (Current)
Prev | E.8 Annexes | Next

### E.8.5 Standard Extended / Specialized / Private SOP Classes

#### E.8.5.1 Standard Extended Basic Film Session SOP Class

The EXAMPLE-PRINT-SERVER-MANAGEMENT is making the following extensions to DICOM SOP Classes:

SOP Class : Basic Film Session SOP

Attribute : Film Destination (2000,0040)

Extensions value : CURRENT

This extension allows the SCU to print on the destination currently configured at the printer.

SOP Class : Basic Film Session SOP

Attribute : Medium Type (2000,2000)

Extensions : CURRENT

This extension allows images to be printed on whatever media type is currently loaded in the printer.

Note that if Medium Type is specified, and a media type other than that requested is installed, then the EXAMPLE-PRINT-SERVER-MANAGEMENT will return success (0x0) and will either queue the print job until the correct media type is installed, or print on the media currently installed, based on the EXAMPLE-PRINT-SERVER-MANAGEMENT configuration. Specifying the Media Type to CURRENT will ensure that the print job will always be printed.

If Medium Type is not specified, then the default CURRENT will be used, allowing images to always be printed.

Prev | Up | Next
E.8.4 Grayscale Image Consistency | Home | E.8.5.2 Standard Extended Basic Film Box SOP Class

DICOM PS3.2 2018e - Conformance