DICOM PS3.3 2018e - Information Object Definitions

F.5.37 Implant Directory Record Definition (Current)
Prev | F.5 Definition of Specific Directory Records | Next

### F.5.37 Implant Directory Record Definition

The Directory Record is based on the specification of Section F.3. It is identified by a Directory Record Type of Value "IMPLANT". Table F.5-37 lists the set of keys with their associated Types for such a Directory Record Type. The description of these keys may be found in the Generic Implant Template IOD. This Directory Record shall be used to reference a Generic Implant Template SOP Instance.

Table F.5-37. Implant Keys

Key | Tag | Type | Attribute Description
--- | --- | --- | ---
Manufacturer | (0008,0070) | 1 | Name of the manufacturer that produces the implant.
Implant Name | (0022,1095) | 1 | The (product) name of the implant.
Implant Size | (0068,6210) | 1C | The size descriptor of the component. Required if present in the referenced instance.
Implant Part Number | (0022,1097) | 1 | The (product) identifier of the implant.

### Note

Because (0004,1511) Referenced SOP Instance UID in File may be used as a "pseudo" Directory Record Key (see Table F.3-3), it is not duplicated in this list of keys.

Prev | Up | Next
F.5.36 Palette Directory Record Definition | Home | F.5.38 Implant Assembly Directory Record Definition

DICOM PS3.3 2018e - Information Object Definitions