DICOM PS3.4 2019a - Service Class Specifications

I.3.2 Conformance as an FSR (Current)
Prev | I.3 Conformance | Next

### I.3.2 Conformance as an FSR

An implementation that conforms to one of the SOP Classes of the Media Storage Service Class:

1. shall meet the requirements specified in Section I.2.2;

2. shall meet the requirements specified in PS3.10;

3. shall perform M-READ Operations according to the SOP Class specification identified by the SOP Class UID in the Meta File Information. M-READ of non-supported SOP Classes shall simply result in ignoring such stored Data Sets;

4. shall read DICOMDIR Files without a Directory Information Module or with a Directory Information Module including Directory Records of a Type not supported by the implementation.

Prev | Up | Next
I.3 Conformance | Home | I.3.3 Conformance as an FSU

DICOM PS3.4 2019a - Service Class Specifications