DICOM PS3.18 2019a - Web Services

6.9.4 RetrieveUPS (Current)
Prev | 6.9 UPS-RS Worklist Service | Next

### 6.9.4 RetrieveUPS

This resource supports the retrieval of a UPS Instance.

#### 6.9.4.1 Request

The request message shall be formed as follows:

- Resource

  - {+SERVICE}/workitems/{UPSInstanceUID}

    where

    - {+SERVICE} is the base URL for the service. This may be a combination of protocol (either HTTP or HTTPS), authority and path.

    - {UPSInstanceUID} is the UID of the Unified Procedure Step Instance

- Method

  - GET

- Headers

  - Accept - The representation scheme in which the RESTful service is requested to return the result. The types allowed for this request header are as follows:

    - application/dicom+xml

      Specifies that the result should be DICOM PS3.19 XML metadata.

    - application/dicom+json

      Specifies that the result should be DICOM PS3.18 JSON metadata.

  - Cache-control: no-cache (recommended)

    If included, specifies that results returned should be current and not cached.

Prev | Up | Next
6.9.3.3.3 Response Message | Home | 6.9.4.2 Behavior

DICOM PS3.18 2019a - Web Services