DICOM PS3.2 2019b - Conformance

D.1 Conformance Statement Overview (Current)
Prev | D Conformance Statement Sample DICOM Image Viewer (Informative) | Next

## D.1 Conformance Statement Overview

The application supports querying a remote system for a list of DICOM objects that may then be retrieved to the local system. It also supports sending locally loaded images across the network to another system.

All storage SOP Classes defined as of DICOM 2002 can be received, stored and transmitted by the application, but only images and spectroscopy objects may be loaded and viewed. All single and multi-frame with grayscale and RGB color (but not palette color, except for Enhanced MR images) images may be displayed.

Only hierarchical query and retrieval is supported.

Table D.1-1. Network Services

SOP Classes | User of Service(SCU) | Provider of Service(SCP)
--- | --- | ---
Transfer |  |
Stored Print Storage SOP Class | Stored only | Yes
Hardcopy Grayscale Image Storage SOP Class | Stored and Viewed | Yes
Hardcopy Color Image Storage SOP Class | Stored and Viewed | Yes
Computed Radiography Image Storage | Stored and Viewed | Yes
Digital X-Ray Image Storage - For Presentation | Stored and Viewed | Yes
Digital X-Ray Image Storage - For Processing | Stored only | Yes
Digital Mammography X-Ray Image Storage - For Presentation | Stored and Viewed | Yes
Digital Mammography X-Ray Image Storage - For Processing | Stored only | Yes
Digital Intra-oral X-Ray Image Storage - For Presentation | Stored and Viewed | Yes
Digital Intra-oral X-Ray Image Storage - For Processing | Stored only | Yes
CT Image Storage | Stored and Viewed | Yes
Ultrasound Multi-frame Image Storage (Retired) | Stored and Viewed | Yes
Ultrasound Multi-frame Image Storage | Stored and Viewed | Yes
MR Image Storage | Stored and Viewed | Yes
Enhanced MR Image Storage | Stored and Viewed | Yes
MR Spectroscopy Storage | Stored and Viewed | Yes
Nuclear Medicine Image Storage (Retired) | Stored and Viewed | Yes
Ultrasound Image Storage (Retired) | Stored and Viewed | Yes
Ultrasound Image Storage | Stored and Viewed | Yes
Secondary Capture Image Storage | Stored and Viewed | Yes
Multi-frame Single Bit Secondary Capture Image Storage | Stored and Viewed | Yes
Multi-frame Grayscale Byte Secondary Capture Image Storage | Stored and Viewed | Yes
Multi-frame Grayscale Word Secondary Capture Image Storage | Stored and Viewed | Yes
Multi-frame True Color Secondary Capture Image Storage | Stored and Viewed | Yes
Standalone Overlay Storage | Stored only | Yes
Standalone Curve Storage | Stored only | Yes
12-lead ECG Waveform Storage | Stored only | Yes
General ECG Waveform Storage | Stored only | Yes
Ambulatory ECG Waveform Storage | Stored only | Yes
Hemodynamic Waveform Storage | Stored only | Yes
Cardiac Electrophysiology Waveform Storage | Stored only | Yes
Basic Voice Audio Waveform Storage | Stored only | Yes
Standalone Modality LUT Storage | Stored only | Yes
Standalone VOI LUT Storage | Stored only | Yes
Grayscale Softcopy Presentation State Storage SOP Class | Stored and Viewed | Yes
X-Ray Angiographic Image Storage | Stored and Viewed | Yes
X-Ray Radiofluoroscopic Image Storage | Stored and Viewed | Yes
X-Ray Angiographic Bi-Plane Image Storage (Retired) | Stored only | Yes
Nuclear Medicine Image Storage | Stored and Viewed | Yes
Raw Data Storage | Stored only | Yes
VL Image Storage (Retired) | Stored and Viewed | Yes
VL Multi-frame Image Storage (Retired) | Stored and Viewed | Yes
VL Endoscopic Image Storage | Stored and Viewed | Yes
VL Microscopic Image Storage | Stored and Viewed | Yes
VL Slide-Coordinates Microscopic Image Storage | Stored and Viewed | Yes
VL Photographic Image Storage | Stored and Viewed | Yes
Basic Text SR | Stored only | Yes
Enhanced SR | Stored only | Yes
Comprehensive SR | Stored only | Yes
Mammography CAD SR | Stored only | Yes
Key Object Selection Document | Stored only | Yes
Positron Emission Tomography Image Storage | Stored and Viewed | Yes
Standalone PET Curve Storage | Stored only | Yes
RT Image Storage | Stored and Viewed | Yes
RT Dose Storage | Stored only | Yes
RT Structure Set Storage | Stored only | Yes
RT Beams Treatment Record Storage | Stored only | Yes
RT Plan Storage | Stored only | Yes
RT Brachy Treatment Record Storage | Stored only | Yes
RT Treatment Summary Record Storage | Stored only | Yes
Query/Retrieve |  |
Study Root Information Model FIND | Yes - Hierarchical only | No
Study Root Information Model MOVE | Yes - Hierarchical only | No

Table D.1-2. Media Services

Media Storage Application Profile | Write Files(FSC or FSU) | Read Files(FSR)
--- | --- | ---
Compact Disk - Recordable |  |
General Purpose CD-R | No | Yes
DVD |  |
General Purpose DVD-RAM | No | Yes

Prev | Up | Next
D Conformance Statement Sample DICOM Image Viewer (Informative) | Home | D.2 Table of Contents

DICOM PS3.2 2019b - Conformance