DICOM PS3.3 2019b - Information Object Definitions

C.8.25.14.5 Ophthalmic Axial Measurements Quality Metric Macro (Current)
Prev | C.8.25.14 Ophthalmic Axial Measurements Module | Next

##### C.8.25.14.5 Ophthalmic Axial Measurements Quality Metric Macro

Table C.8.25.14-6 describes the Attributes for the Ophthalmic Axial Length Quality Metric Macro.

Table C.8.25.14-6. Ophthalmic Axial Length Quality Metric Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Concept Name Code Sequence | (0040,A043) | 1 | Type of metric used to evaluate the quality of the ophthalmic axial length. Only a single Item shall be included in this Sequence.
>Include Table 8.8-1 “Code Sequence Macro Attributes” | DCID 4243 “Ophthalmic Quality Metric Type”
Numeric Value | (0040,A30A) | 1 | Value for quality metric applied to axial length values.
Measurement Units Code Sequence | (0040,08EA) | 1 | Units of Numeric Value (0040,A30A). Only a single Item shall be included in this Sequence.
>Include Table 8.8-1 “Code Sequence Macro Attributes” | DCID 82 “Units of Measurement”.

Prev | Up | Next
C.8.25.14.4 Ophthalmic Axial Measurements Selected Macro | Home | C.8.25.15 Intraocular Lens Calculations Series Module

DICOM PS3.3 2019b - Information Object Definitions