DICOM PS3.17 2019c - Explanatory Information

JJJJ Multi-energy CT Imaging (Informative) (Current)
Prev |  | Next

# JJJJ Multi-energy CT Imaging (Informative)

## JJJJ.1 Domain of Application

Multi-energy CT acquires pixel information which correlates to different X-Ray spectra to enable differentiation, quantification and classification of different types of tissues.

To detect the different X-Ray spectra, Multi-energy (ME) CT imaging uses combinations of different Source(s) and Detector(s) technologies such as current switching X-Ray tubes, spectral detectors, multi-layer detectors, multi-source and detector pairs.

Prev |  | Next
IIII.2 Example of Fused CT/MR Derived Encapsulated STL | Home | JJJJ.2 Use Cases

DICOM PS3.17 2019c - Explanatory Information