DICOM PS3.3 2019c - Information Object Definitions

C.8.31.7 X-Ray Grid Macro (Current)
Prev | C.8.31.6 Breast X-Ray Isocenter Reference System Macro | Next

##### C.8.31.7 X-Ray Grid Macro

Table C.8.31.7-1 specifies the Attributes of the X-Ray Grid Functional Group Macro.

Table C.8.31.7-1. X-Ray Grid Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
X-Ray Grid Sequence | (0018,9555) | 1 | A Sequence that describes the geometrical position of the positioner. Only a single Item shall be included in this Sequence.
>Grid | (0018,1166) | 1 | Identified the grid. May be multi-valued. Defined Terms: FIXED FOCUSED RECIPROCATING PARALLEL CROSSED NONE
Include Table C.8-36b “X-Ray Grid Description Macro Attributes” |

Prev | Up | Next
C.8.31.6 Breast X-Ray Isocenter Reference System Macro | Home | C.8.31.8 X-Ray Filter Macro

DICOM PS3.3 2019c - Information Object Definitions