DICOM PS3.3 2019c - Information Object Definitions

C.8.20 Segmentation (Current)
Prev | C.8 Modality Specific Modules | Next

### C.8.20 Segmentation

This section describes the specific Modules for the Segmentation IOD.

#### C.8.20.1 Segmentation Series Module

Table C.8.20-1 defines the general Attributes of the Segmentation Series Module.

Table C.8.20-1. Segmentation Series Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Modality | (0008,0060) | 1 | Modality type Enumerated Values: SEG
Series Number | (0020,0011) | 1 | A number that identifies this Series
Referenced Performed Procedure Step Sequence | (0008,1111) | 1C | Uniquely identifies the Performed Procedure Step SOP Instance to which the Series is related Only a single Item shall be included in this Sequence. Required if a Performed Procedure Step SOP Class was involved in the creation of this Series.
>Include Table 10-11 “SOP Instance Reference Macro Attributes” |

Prev | Up | Next
C.8.19.7 XA/XRF Multi-frame Presentation Module | Home | C.8.20.2 Segmentation Image Module

DICOM PS3.3 2019c - Information Object Definitions