DICOM PS3.3 2019e - Information Object Definitions

A.74.3 Breast Projection X-Ray Image IOD Module Table (Current)
Prev | A.74 Breast Projection X-Ray Image IOD | Next

### A.74.3 Breast Projection X-Ray Image IOD Module Table

Table A.74-1 specifies the Modules of the Breast Projection X-Ray Image IOD.

Table A.74-1. Breast Projection X-Ray Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
DX Series | C.8.11.1 | M
Enhanced Mammography Series | C.8.11.10 | M
Frame of Reference | Frame of Reference | C.7.4.1 | M
Synchronization | C.7.4.2 | C - Required if time synchronization was applied.
Equipment | General Equipment | C.7.5.1 | M
Enhanced General Equipment | C.7.5.2 | M
Image | Enhanced Mammography Image | C.8.31.1 | M
Breast View | C.8.21.6 | M
Image Pixel | C.7.6.3 | M
Enhanced Contrast/Bolus | C.7.6.4b | C - Required if contrast media was applied.
Device | C.7.6.12 | U
Intervention | C.7.6.13 | U
Acquisition Context | C.7.6.14 | M
Multi-frame Functional Groups | C.7.6.16 | M
Multi-frame Dimension | C.7.6.17 | U
Patient Orientation | C.7.6.20 | M
Specimen | C.7.6.22 | U
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U
Frame Extraction | C.12.3 | C - Required if the SOP Instance was created in response to a Frame-Level retrieve request

#### A.74.3.1 Breast Projection X-Ray Image IOD Content Constraints

##### A.74.3.1.1 Modality Attribute

Modality (0008,0060) shall have the value MG.

##### A.74.3.1.2 Overlay Plane Module, Curve Module and VOI LUT Module

The Overlay Plane Module, Curve Module (Retired), VOI LUT Module and Softcopy Presentation LUT Module shall not be used in a Standard Extended SOP Class of the Breast Projection X-Ray Image.

### Note

The VOI LUT function is provided by a Frame VOI LUT Functional Group.

Prev | Up | Next
A.74.2 Breast Projection X-Ray Image IOD Entity-Relationship Model | Home | A.74.4 Breast Projection X-Ray Image Functional Group Macros

DICOM PS3.3 2019e - Information Object Definitions