DICOM PS3.3 2019e - Information Object Definitions

A.55.4 Breast Tomosynthesis Image Functional Group Macros (Current)
Prev | A.55 Breast Tomosynthesis Image IOD | Next

### A.55.4 Breast Tomosynthesis Image Functional Group Macros

Table A.55-2 specifies the use of the Functional Group Macros used in the Multi-frame Functional Groups Module for the Breast Tomosynthesis Image IOD.

Table A.55-2. Breast Tomosynthesis Image Functional Group Macros

Functional Group Macro | Section | Usage
--- | --- | ---
Pixel Measures | C.7.6.16.2.1 | M
Frame Content | C.7.6.16.2.2 | M - May not be used as a Shared Functional Group.
Plane Position (Patient) | C.7.6.16.2.3 | M
Plane Orientation (Patient) | C.7.6.16.2.4 | M
Referenced Image | C.7.6.16.2.5 | U
Derivation Image | C.7.6.16.2.6 | C - Required if Image Type (0008,0008) Value 1 equals DERIVED.
Frame Anatomy | C.7.6.16.2.8 | M
Identity Pixel Value Transformation | C.7.6.16.2.9b | M
Frame VOI LUT With LUT | C.7.6.16.2.10b | M
Real World Value Mapping | C.7.6.16.2.11 | U
Contrast/Bolus Usage | C.7.6.16.2.12 | C - Required if the Enhanced Contrast/Bolus Module is present.
X-Ray 3D Frame Type | C.8.21.5.1 | M - May not be used as a Shared Functional Group.
Breast Biopsy Target | C.8.21.5.2 | U – May not be used as a Shared Functional Group.

#### A.55.4.1 Breast Tomosynthesis Image Functional Group Macros Content Constraints

##### A.55.4.1.1 Frame Anatomy Functional Group Macro

The Defined CID for the Anatomic Region Sequence (0008,2218) shall be CID 4013 “Anatomic Region for Mammography”.

Prev | Up | Next
A.55.3 Breast Tomosynthesis Image IOD Module Table | Home | A.56 Enhanced PET Image IOD

DICOM PS3.3 2019e - Information Object Definitions