DICOM PS3.17 2019e - Explanatory Information

HH Segmentation Encoding Example (Informative) (Current)
Prev |  | Next

# HH Segmentation Encoding Example (Informative)

Figure HH-1 depicts an example of how the data is organized within an instance of the Segmentation IOD. Each item in the Segment Sequence provides the Attributes of a segment. The source image used in all segmentations is referenced in the Shared Functional Groups Sequence. Each item of the Per-frame Functional Groups Sequence maps a frame to a segment. The Pixel Data classifies the corresponding pixels/voxels of the source Image.

Figure HH-1. Segment Sequence Structure and References

Prev |  | Next
GG JPIP Referenced Pixel Data Transfer Syntax Negotiation (Informative) | Home | II Use of Product Characteristics Attributes in Composite SOP Instances (Informative)

DICOM PS3.17 2019e - Explanatory Information