DICOM PS3.17 2019e - Explanatory Information

XXX.3.12.3 Encoding Details (Current)
Prev | XXX.3.12 Liver Resection Planning | Next

#### XXX.3.12.3 Encoding Details

##### XXX.3.12.3.1 Volumetric Presentation State Relatonship Module Recommendations

Table XXX.3.12.3.1-1. Volumetric Presentation State Relatonship Module Recommendations

Attribute Name | Tag | Comment
Volumetric Presentation Input Set Sequence | (0070,120A) |
Item #1
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID1
>Presentation Input Type | (0070,1202) | Set to VOLUME
>Referenced Image Sequence | (0008,1140) | Reference to Arterial phase CT volume
Item #2
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID2
>Presentation Input Type | (0070,1202) | Set to VOLUME
>Referenced Image Sequence | (0008,1140) | Reference to Portal Venous phase CT volume
Volumetric Presentation State Input Sequence | (0070,1201) |
Item #1
>Volumetric Presentation Input Number | (0070,1207) | Set to 1
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID1
>Include VOI LUT Macro Table C.11-2B | Set to identity
>Crop | (0070,1204) | Set to YES
>Cropping Specification Index | (0070,1205) | Set to 1
Item #2
>Volumetric Presentation Input Number | (0070,1207) | Set to 2
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID1
>Include VOI LUT Macro Table C.11-2B | Set to identity
>Crop | (0070,1204) | Set to YES
>Cropping Specification Index | (0070,1205) | Set to 2
Item #3
>Volumetric Presentation Input Number | (0070,1207) | Set to 3
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID1
>Include VOI LUT Macro Table C.11-2B | Set to identity
>Crop | (0070,1204) | Set to YES
>Cropping Specification Index | (0070,1205) | Set to 3
Item #4
>Volumetric Presentation Input Number | (0070,1207) | Set to 4
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID2
>Include VOI LUT Macro Table C.11-2B | Set to identity
>Crop | (0070,1204) | Set to YES
>Cropping Specification Index | (0070,1205) | Set to 4
Item #5
>Volumetric Presentation Input Number | (0070,1207) | Set to 5
>Volumetric Presentation Input Set UID | (0070,1209) | Set to UID2
>Include VOI LUT Macro Table C.11-2B | Set to identity
>Crop | (0070,1204) | Set to YES
>Cropping Specification Index | (0070,1205) | Set to 5

Prev | Up | Next
XXX.3.12.2 Encoding Outline | Home | XXX.3.12.3.2 Volume Cropping Module Recommendations

DICOM PS3.17 2019e - Explanatory Information