DICOM PS3.4 2019e - Service Class Specifications

J.3.6.2.2 Notifications (Current)
Prev | J.3.6.2 SCP Conformance. | Next

##### J.3.6.2.2 Notifications

The SCP shall document in the SCP Notifications Statement the behavior and actions that cause the SCP to generate an N-EVENT-REPORT primitive (Storage Commitment Result).

The SCP shall specify if it supports the optional Storage Media File-Set ID & UID Attributes in the N-EVENT-REPORT and describe the policies for how the Media is used. The SCP shall also specify which Storage Media Application Profiles are supported.

The SCP shall specify if it supports the optional Retrieve AE Title (0008,0054) Attribute in the N-EVENT-REPORT and describe the policies for how it is used.

The SCP Notifications Statement shall be formatted as defined in PS3.2

Prev | Up | Next
J.3.6.2 SCP Conformance. | Home | J.4 Storage Commitment Pull Model SOP Class(Retired)

DICOM PS3.4 2019e - Service Class Specifications