DICOM PS3.3 2019e - Information Object Definitions

A.65.3 Ophthalmic Visual Field Static Perimetry Measurements IOD Modules (Current)
Prev | A.65 Ophthalmic Visual Field Static Perimetry Measurements IOD | Next

### A.65.3 Ophthalmic Visual Field Static Perimetry Measurements IOD Modules

Table A.65.3-1 specifies the Modules of the Ophthalmic Visual Field Static Perimetry Measurements IOD.

Table A.65.3-1. Ophthalmic Visual Field Static Perimetry Measurements IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Visual Field Static Perimetry Measurements Series | C.8.26.1 | M
Equipment | General Equipment | C.7.5.1 | M
Enhanced General Equipment | C.7.5.2 | M
Measurements | Visual Field Static Perimetry Test Parameters | C.8.26.2 | M
Visual Field Static Perimetry Test Reliability | C.8.26.3 | M
Visual Field Static Perimetry Test Measurements | C.8.26.4 | M
Visual Field Static Perimetry Test Results | C.8.26.5 | M
Ophthalmic Patient Clinical Information and Test Lens Parameters | C.8.26.6 | U
SOP Common | C.12.1 | M

Prev | Up | Next
A.65.2 Ophthalmic Visual Field Static Perimetry Measurements IOD Entity-Relationship Model | Home | A.66 Intravascular OCT IOD

DICOM PS3.3 2019e - Information Object Definitions