DICOM PS3.4 2019e - Service Class Specifications

H.3.2 Print Management Meta SOP Classes (Current)
Prev | H.3 Print Management Conformance | Next

### H.3.2 Print Management Meta SOP Classes

#### H.3.2.1 Description

The Basic Print Management Meta SOP Classes correspond with the minimum functionality that an implementation of the Print Management Service Class shall support. The Basic Print Management Meta SOP Classes support the following mandatory features:

- preformatted grayscale images or preformatted color images; preformatted images are images where annotation, graphics, overlays are burned in

- pre-defined film layouts (image display formats)

- basic presentation parameters on film session, film box and image box level

- basic device management

The optional SOP Classes described in Section H.3.3 may be used with the Basic Print Management Meta SOP Classes.

The following features are optional for SCUs and SCPs:

- Film box annotation

- Presentation LUT

Prev | Up | Next
H.3 Print Management Conformance | Home | H.3.2.2 Meta SOP Class Definitions

DICOM PS3.4 2019e - Service Class Specifications