DICOM PS3.3 2019e - Information Object Definitions

C.36.2.2 RT Second Generation Device Macros (Current)
Prev | C.36.2 RT Second Generation Macros | Next

#### C.36.2.2 RT Second Generation Device Macros

##### C.36.2.2.1 Treatment Device Identification Macro

The Treatment Device Identification Macro identifies a device used to deliver radiation to the patient during a radiotherapy treatment session.

Table C.36.2.2.1-1. Treatment Device Identification Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Treatment Device Identification Sequence | (300A,063A) | 1 | Identifies treatment device. Only a single Item shall be included in this Sequence.
>Include Table 10.35-1 “Device Model Macro Attributes”. | Identifies the device model for the Treatment Device.
>Manufacturer's Device Class UID | (0018,100B) | 2 | Manufacturer's Unique Identifier (UID) for the class of the device. A class is a manufacturer-specific grouping concept with no DICOM-defined scope or criteria. A class is independent from a marketing-defined make, model or version. A class allows definition of a group of devices with a similar set of capabilities.
>Include Table 10.36-1 “Device Identification Macro Attributes”. | DCID 9551 “Treatment Delivery Device Types”.
>Institution Name | (0008,0080) | 3 | Institution where the equipment is located.
>Institution Address | (0008,0081) | 3 | Mailing address of the institution where the equipment is located.
>Institutional Department Name | (0008,1040) | 3 | Department in the institution where the equipment is located.

Prev | Up | Next
C.36.2 RT Second Generation Macros | Home | C.36.2.2.2 RT Patient Support Devices Macro

DICOM PS3.3 2019e - Information Object Definitions