DICOM PS3.3 2019e - Information Object Definitions

C.32.3.2 Visual Evaluation Result Macro (Current)
Prev | C.32.3 QA Results Module | Next

#### C.32.3.2 Visual Evaluation Result Macro

This Macro records the result of a Visual Evaluation QA task by a human for a Display System.

Table C.32.3.2-1. Visual Evaluation Result Macro Attributes

Attribute Name | Tag | Description
--- | --- | ---
Visual Evaluation Test Sequence | (0028,7028) | Test Results of a visual evaluation of the display subsystem output. May include evaluation of multiple test pattern images, as long as all Items in this Sequence are generated in a single QA test session. One or more Items shall be included in this Sequence.
>Test Result | (0028,7029) | Result of a test. Enumerated Values: PASS Evaluated as acceptable FAIL Evaluated as not acceptable SKIP Not evaluated
>Test Result Comment | (0028,702A) | User comment on the result or performance of the test. Might include scoring values that are not intended to be machine readable.
>Test Pattern Code Sequence | (0028,702C) | Coded identification of the test pattern presented for visual evaluation. Only a single Item shall be included in this Sequence.
>>Include Table 8.8-1 “Code Sequence Macro Attributes” | BCID 8301 “Test Pattern Codes”.
>Referenced Image Sequence | (0008,1140) | Reference to the image instance containing the test pattern presented for visual evaluation. Only a single Item shall be included in this Sequence. Required if Test Pattern Code Sequence (0028,702C) is absent in this Item. May be present otherwise.
>>Test Image Validation | (0028,702B) | Indication of whether the test image was validated as matching the characteristics of the display system (e.g., resolution and bit depth). Enumerated Values: MATCHED the test image was determined to match UNMATCHED the test image was not determined to match
Visual Evaluation Method Code Sequence | (0028,702E) | Coded description of the methodology used during this visual evaluation. Only a single Item shall be included in this Sequence.
>Include Table 8.8-1 “Code Sequence Macro Attributes” | BCID 8300 “Visual Evaluation Methods”.

Prev | Up | Next
C.32.3 QA Results Module | Home | C.32.3.3 Luminance Uniformity Result Macro

DICOM PS3.3 2019e - Information Object Definitions