DICOM PS3.4 2020a - Service Class Specifications

FF.2.4.2.3 Crosscurve Animation (Current)
Prev | FF.2.4.2 Volumetric Animation | Next

##### FF.2.4.2.3 Crosscurve Animation

A Presentation Animation Style (0070,1A01) value of CROSSCURVE indicates that Crosscurve Animation is being specified. In this animation style, a Presentation State defines a Planar MPR view at the beginning of a curve defined in Animation Curve Sequence (0070,1A04). The Planar MPR view is stepped a distance Animation Step Size (0070,1A05) along the curve defined in Animation Curve Sequence (0070,1A04) at the rate specified by Recommended Animation Rate (0070,1A03) in steps per second. See Figure FF.3.2-3.

### Note

A typical application of this animation style is motion along a curve centered within the colon or a blood vessel.

Figure FF.3.2-3. Crosscurve Animation

Prev | Up | Next
FF.2.4.2.2 Presentation Sequence Animation | Home | FF.2.4.2.4 Flythrough Animation

DICOM PS3.4 2020a - Service Class Specifications