DICOM PS3.17 2020a - Explanatory Information

U.2 Typical Sequence of Events (Current)
Prev | U Ophthalmology Use Cases (Informative) | Next

## U.2 Typical Sequence of Events

The following shows the proposed sequence of events using individual images that are captured for later stereo viewing, with the stereo viewing relationships captured in the stereometric relationship instance.

Figure U.2-1. Typical Sequence of Events

The instances captured are all time stamped so that the fluorescein progress can be measured accurately. The acquisition and equipment information captures the different setups that are in use:

1. Acquisition information A is the ordinary illumination and planned lenses for the examination.

2. Acquisition information B is the filtered illumination, filtered viewing, and lenses appropriate for the fluorescein examination.

3. Acquisition information C indicates no change to the equipment settings, but once the injection is made, the subsequent images include the drug, method, dose, and time of delivery.

Prev | Up | Next
U Ophthalmology Use Cases (Informative) | Home | U.3 Ophthalmic Tomography Use Cases (Informative)

DICOM PS3.17 2020a - Explanatory Information