DICOM PS3.16 2020a - Content Mapping Resource

TID 3209 Centerline Wall Motion (Current)
Prev | Quantitative Ventricular Analysis Report SR IOD Templates | Next

### TID 3209 Centerline Wall Motion

The Centerline Wall Motion Template consists of a CONTAINER providing measurements of the centerline wall motion.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3209. Centerline Wall Motion

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (121070, DCM, "Findings") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (111004, DCM, "Analysis Performed") | 1 | M |  | EV (122449, DCM, "Centerline Wall Motion Analysis")
3 | >> | HAS CONCEPT MOD | CODE | EV (122410, DCM, "Contour Realignment") | 1 | M |  | DCID 3458 “Contour Realignment”
4 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 100 | M |  | $Measurement = EV (122450, DCM, "Normalized Chord Length") $Unit = DT (%, UCUM, "%")
5 | > | CONTAINS | NUM | EV (122411, DCM, "Threshold Value") | 1 | M |  | Values shall be 1, 2 or 3 UNITS = EV ({sd}, UCUM, "Standard Deviations")
6 | > | CONTAINS | CONTAINER | EV (122451, DCM, "Abnormal Region") | 1-6 | U |  |
7 | >> | CONTAINS | CODE | EV (60797005, SCT, "Cardiac Wall Motion") | 1 | M |  | DCID 3703 “Wall Motion”
8 | >> | CONTAINS | CODE | EV (255593009, SCT, "Circumferential Extent") | 1 | U |  | DCID 3460 “Circumferential Extent”
9 | >> | CONTAINS | NUM | EV (122452, DCM, "First Chord of Abnormal Region") | 1 | M |  | Unit = DT (1, UCUM, "no unit")
10 | >> | CONTAINS | NUM | EV (122453, DCM, "Last Chord of Abnormal Region") | 1 | M |  | Unit = DT (1, UCUM, "no unit")
11 | > | CONTAINS | CONTAINER | EV (122417, DCM, "Regional Abnormal Wall Motion ") | 1-4 | U |  |
12 | >> | HAS CONCEPT MOD | CODE | EV (363698007, SCT, "Finding Site") | 1 | M |  | DCID 3461 “Regional Extent”
13 | >> | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (122459, DCM, "Territory Region Severity") $ModType = EV (60797005, SCT, "Cardiac Wall Motion") $ModValue = DCID 3703 “Wall Motion” $Unit = DT ({sd}, UCUM, "Standard Deviations")
14 | >> | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (122461, DCM, "Opposite Region Severity") $ModType = EV (60797005, SCT, "Cardiac Wall Motion") $ModValue = DCID 3703 “Wall Motion” $Unit = DT ({sd}, UCUM, "Standard Deviations")
15 | > | CONTAINS | IMAGE |  | 1 | U |  |

Content Item Descriptions

Row 4 | Normalized lengths of the chords determined between ED and ES contour. The measurement Template allows the specification of the statistical properties of the normal population and of the chord measurement relative to the population.
Row 8 | If the Circumferential Extent is not specified no limitations to the boundaries for regions are assumed.
Row 11 | The Regional Abnormal Wall Motion container holds the information on the severity of the decreased or increased wall motion of the 4 predefined regions as described in [Sheehan, 1986].
Row 12 | The name of the region with an abnormal ventricular wall motion as described in [Sheehan, 1986].
Row 13 | The severity of the wall motion abnormality expressed in Standard Deviations above or below normal in the territory region as described in [Sheehan, 1986].
Row 14 | The severity of the wall motion abnormality expressed in Standard Deviations above or below normal in the opposite region as described in [Sheehan, 1986].
Row 15 | Secondary Capture image with centerline analysis result. No purpose of reference is specified.

Prev | Up | Next
TID 3208 Frame-to-Frame Results | Home | TID 3210 Radial Based Wall Motion

DICOM PS3.16 2020a - Content Mapping Resource