DICOM PS3.3 2020a - Information Object Definitions

C.14 Storage Commitment Module (Current)
Prev | C Information Module Definitions (Normative) | Next

## C.14 Storage Commitment Module

Table C.14-1 defines the Attributes for referencing SOP Instances that are contained in a Storage Commitment Request/Response.

Table C.14-1. Storage Commitment Module Attributes

Attribute Name | Tag | Attribute Description
--- | --- | ---
Transaction UID | (0008,1195) | Uniquely identifies this Storage Commitment transaction.
Retrieve AE Title | (0008,0054) | Application Entity Title where the SOP Instance(s) may be retrieved via a network based retrieve service.
Storage Media File-Set ID | (0088,0130) | User or implementation specific human readable identification of a Storage Media on which the SOP Instances reside.
Storage Media File-Set UID | (0088,0140) | Uniquely identifies a Storage Media on which the SOP Instances reside.
Referenced SOP Sequence | (0008,1199) | A Sequence of Items where each Item references a single SOP Instance for which storage commitment is requested / or has been provided.
>Include Table 10-11 “SOP Instance Reference Macro Attributes” |
>Retrieve AE Title | (0008,0054) | Application Entity Title from which the SOP Instance may be retrieved via a network based retrieve service.
>Storage Media File-Set ID | (0088,0130) | The user or implementation specific human readable identifier that identifies a Storage Media on which this SOP Instance resides.
>Storage Media File-Set UID | (0088,0140) | Uniquely identifies a Storage Media on which this SOP Instance resides.
Failed SOP Sequence | (0008,1198) | A Sequence of Items where each Item references a single SOP Instance for which storage commitment could not be provided.
>Include Table 10-11 “SOP Instance Reference Macro Attributes” |
>Failure Reason | (0008,1197) | The reason that storage commitment could not be provided for this SOP Instance. See Section C.14.1.1.

### Note

1. Conditions under which Attributes are required (i.e., Retrieve AE Title, etc.) are defined in the Storage Commitment Service Class in PS3.4.

2. Referenced Performed Procedure Step Sequence (0008,1111) was included in this Module in earlier versions, but its use here has been retired. See PS3.4-2001, in which the Attribute was formerly known as Referenced Study Component Sequence.

### C.14.1 Storage Commitment Attribute Description

#### C.14.1.1 Failure Reason

The following values and semantics shall be used for Failure Reason (0008,1197):

Enumerated Values:

0110H

  Processing failure

  A general failure in processing the operation was encountered.

0112H

  No such object instance

  One or more of the elements in the Referenced SOP Instance Sequence was not available.

0213H

  Resource limitation

  The SCP does not currently have enough resources to store the requested SOP Instance(s).

0122H

  Referenced SOP Class not supported

  Storage Commitment has been requested for a SOP Instance with a SOP Class that is not supported by the SCP.

0119H

  Class/Instance conflict

  The SOP Class of an element in the Referenced SOP Instance Sequence did not correspond to the SOP class registered for this SOP Instance at the SCP.

0131H

  Duplicate transaction UID

  The Transaction UID of the Storage Commitment Request is already in use.

Prev | Up | Next
C.13.13 Printer Configuration Module | Home | C.15 Queue Management Specific Modules

DICOM PS3.3 2020a - Information Object Definitions