DICOM PS3.3 2020a - Information Object Definitions

A.27.3 Digital Mammography X-Ray Image IOD Module Table (Current)
Prev | A.27 Digital Mammography X-Ray Image IOD | Next

### A.27.3 Digital Mammography X-Ray Image IOD Module Table

Table A.27-1 specifies the Modules of the Digital Mammography X-Ray Image IOD.

Table A.27-1. Digital Mammography X-Ray Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
DX Series | C.8.11.1 | M
Mammography Series | C.8.11.6 | M
Frame of Reference | Frame of Reference | C.7.4.1 | C - Required if multiple images are obtained without releasing breast compression
Equipment | General Equipment | C.7.5.1 | M
Image | General Image | C.7.6.1 | M
General Reference | C.12.4 | U
Image Pixel | C.7.6.3 | M
Contrast/Bolus | C.7.6.4 | U
Display Shutter | C.7.6.11 | U
Device | C.7.6.12 | U
Intervention | C.7.6.13 | U
Specimen | C.7.6.22 | U
DX Anatomy Imaged | C.8.11.2 | M
DX Image | C.8.11.3 | M
DX Detector | C.8.11.4 | M
X-Ray Collimator | C.8.7.3 | U
DX Positioning | C.8.11.5 | U
X-Ray Tomography Acquisition | C.8.7.7 | U
X-Ray Acquisition Dose | C.8.7.8 | U
X-Ray Generation | C.8.7.9 | U
X-Ray Filtration | C.8.7.10 | U
X-Ray Grid | C.8.7.11 | U
Mammography Image | C.8.11.7 | M
Overlay Plane | C.9.2 | C - Required if graphic annotation is present - See Section A.27.3
VOI LUT | C.11.2 | C - Required if Presentation Intent Type (0008,0068) is FOR PRESENTATION. Shall not be present otherwise.
Image Histogram | C.11.5 | U
Acquisition Context | C.7.6.14 | M
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U

### Note

1. The Curve Module (Retired) was previously included in this IOD but has been retired. See PS3.3-2004.

2. The Specimen Identification Module was previously included in this IOD but has been retired, and its functionality replaced by the Specimen Module. See PS3.3-2008.

Prev | Up | Next
A.27.2 Digital Mammography X-Ray Image IOD Entity-Relationship Model | Home | A.27.4 Overlay Plane Module

DICOM PS3.3 2020a - Information Object Definitions