DICOM PS3.18 2020b - Web Services

8.7.2 DICOM Resource Categories (Current)
Prev | 8.7 Media Types | Next

### 8.7.2 DICOM Resource Categories

Table 8.7.2-1 defines Resource Categories that correspond to different SOP Classes. The following sections map each Resource Category to appropriate DICOM and Rendered media types.

Table 8.7.2-1. Resource Categories

Resource Category | Definition
--- | ---
Single Frame Image | This category includes all resources that are: Instances of a single frame SOP Class, or Instances of a multi-frame SOP Class that contain only one frame, or a single frame selected from an Instance of a multi-frame SOP Class.
Multi-Frame Image | This category includes all resources that are Instances of a multi-frame SOP Class, that are not Video and that contain more than one frame.
Video | This category includes all resources that contain more than one frame and are: Instances encoded in the MPEG family of Transfer Syntaxes (which includes MP4 and H.265), or time-based (motion) multi-frame images that the origin server is capable of encoding in the MPEG family.
Text | This category includes all resources that contain: the SR Document Content Module (see Section C.17.3 “SR Document Content Module” in PS3.3), such as narrative text, Structured Reports, CAD, measurement reports, and key object selection documents, or the Encapsulated Document Module (see Section C.24.2 “Encapsulated Document Module” in PS3.3).
Other | This category includes all resources that are not included above, for example waveforms.

Prev | Up | Next
8.7 Media Types | Home | 8.7.3 DICOM Media Types and Media Types For Bulkdata

DICOM PS3.18 2020b - Web Services