DICOM PS3.3 2020b - Information Object Definitions

C.36.2.2.2 RT Patient Support Devices Macro (Current)
Prev | C.36.2.2 RT Second Generation Device Macros | Next

##### C.36.2.2.2 RT Patient Support Devices Macro

The RT Patient Support Devices Macro identifies a patient support device (table, table top, chair or similar) which shall be used for treatment.

Table C.36.2.2.2-1. RT Patient Support Devices Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Number of Patient Support Devices | (300A,0687) | 1 | Number of Patient Support Devices defined in the Patient Support Devices Sequence (300A,0686).
Patient Support Devices Sequence | (300A,0686) | 1C | Patient support device definitions. Required if the Number of Patient Support Devices (300A,0687) is non-zero. The number of Items included in this Sequence shall equal the value ofNumber of Patient Support Devices (300A,0687).
>Device Index | (3010,0039) | 1 | Index of the Device in this Sequence. The value shall start at 1 and increase monotonically by 1.
>Include Table 10.35-1 “Device Model Macro Attributes”.
>Include Table 10.36-1 “Device Identification Macro Attributes”. | DCID 9505 “Fixation or Positioning Devices”.
>Conceptual Volume Sequence | (3010,0025) | 2 | References a conceptual volume that describes the geometry and properties of the patient support device. Zero or one Item shall be included in this Sequence.
>>Include Table 10.34-1 “Conceptual Volume Segmentation Reference And Combination Macro Attributes”.

Prev | Up | Next
C.36.2.2 RT Second Generation Device Macros | Home | C.36.2.2.3 RT Accessory Device Identification Macro

DICOM PS3.3 2020b - Information Object Definitions