DICOM PS3.3 2020c - Information Object Definitions

C.11.25 Presentation View Description Module (Current)
Prev | C.11 Look Up Tables and Presentation States | Next

### C.11.25 Presentation View Description Module

Table C.11.25-1 contains Attributes that describe the view of this presentation in anatomical terms.

Note: For example, a Volumetric Presentation State derived from a whole-body CT source volume could be restricted to the left leg.

Table C.11.25-1. Presentation View Description Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Include Table 10-6 “General Anatomy Required Macro Attributes” | No Baseline CID is defined.
View Code Sequence | (0054,0220) | 2 | Describes this view of the patient anatomy. No more than one Item shall be included in this Sequence.
>Include Table 8.8-1 “Code Sequence Macro Attributes” . | BCID 501 “Volumetric View Description”.
>View Modifier Code Sequence | (0054,0222) | 2 | View modifier. Zero or more Items shall be included in this Sequence.
>> Include Table 8.8-1 “Code Sequence Macro Attributes” . | BCID 502 “Volumetric View Modifier”.
Image Laterality | (0020,0062) | 2 | Laterality of (possibly paired) body part (as described in Anatomic Region Sequence (0008,2218) ) examined. Enumerated Values: R right L left U unpaired B both left and right Shall be consistent with any laterality information contained in Primary Anatomic Structure Modifier Sequence (0008,2230), if present.

Prev | Up | Next
C.11.24 Volume Cropping Module | Home | C.11.26 Multi-Planar Reconstruction Geometry Module

DICOM PS3.3 2020c - Information Object Definitions