DICOM PS3.16 2020c - Content Mapping Resource

CID 71 Imaging Agent Administration Injector Event Type (Current)
Prev | B DCMR Context Groups (Normative) | Next

## CID 71 Imaging Agent Administration Injector Event Type

Resources:

  HTML | FHIR JSON | FHIR XML | IHE SVS XML

Type:

  Extensible

Version:

  20181115

UID:

  1.2.840.10008.6.1.1261

Table CID 71. Imaging Agent Administration Injector Event Type

Coding Scheme Designator | Code Value | Code Meaning
--- | --- | ---
DCM | 130150 | Pressure above warning limit
DCM | 130151 | Pressure above adjustment limit
DCM | 130152 | Flow rate above warning limit
DCM | 130153 | Flow rate above adjustment limit
DCM | 130161 | Keep vein open started
DCM | 130162 | Keep vein open ended
DCM | 130175 | Air detected
DCM | 130155 | Fixed duration pause ended
DCM | 130163 | Syringe attached
DCM | 130164 | Syringe detached
DCM | 110501 | Equipment failure
DCM | 110527 | Resource inadequate
DCM | 130156 | Terminated due to pressure above termination limit
DCM | 130157 | Terminated due to flow rate above termination limit
DCM | 130176 | Terminated due to air detected
DCM | 130158 | Terminated due to excessive duration pause
DCM | 130154 | Terminated due to request from operator
DCM | 130159 | Terminated due to injector communication loss
DCM | 130160 | Terminated due to unspecified injector failure
DCM | 130177 | Terminated by scanner
DCM | 130178 | Terminated due to critical battery level
DCM | 130179 | Terminated due to consumable removal

Prev | Up | Next
CID 70 Flush | Home | CID 72 Imaging Agent Administration Step Type

DICOM PS3.16 2020c - Content Mapping Resource