DICOM PS3.17 2020c - Explanatory Information

XXX.3.7.3.3 Multi-Planar Reconstruction Geometry Module Recommendations (Current)
Prev | XXX.3.7.3 Encoding Details | Next

##### XXX.3.7.3.3 Multi-Planar Reconstruction Geometry Module Recommendations

Table XXX.3.7-3. Multi-Planar Reconstruction Geometry Module Recommendations

Attribute Name | Tag | Comment
--- | --- | ---
Multi-Planar Reconstruction Style | (0070,1501) | Set to PLANAR
MPR Thickness Type | (0070,1502) | Set to THIN
MPR View Width Direction | (0070,1507) | Set to the direction of the top row of the MPR view in the VPC-RCS
MPR View Width | (0070,1508) | Set to the width of the top row of the MPR view in the VPC-RCS
MPR View Height Direction | (0070,1511) | Set to the direction of the leftmost column of the MPR view in the VPC-RCS
MPR View Height | (0070,1512) | Set to the width of the leftmost column of the MPR view in the VPC-RCS
MPR Top Left Hand Corner | (0070,1505) | Set to an (x,y,z) point in the VPC-RCS of the upper left corner of the MPR view

Prev | Up | Next
XXX.3.7.3.2 Presentation View Description Module Recommendations | Home | XXX.3.7.3.4 Volumetric Presentation State Display Module Recommendations

DICOM PS3.17 2020c - Explanatory Information