DICOM PS3.16 2020c - Content Mapping Resource

TID 10031 Radiation Dose Estimate (Current)
Prev | Patient Radiation Dose SR IOD Templates | Next

### TID 10031 Radiation Dose Estimate

The dose estimate is used to record the results from one analysis method from one or more radiation sources. Organ dose estimates are calculated from one or more irradiation events to a patient. The output from one or more sources of radiation can be used separately or combined to estimate the dose to a patient or individual organs.

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 10031. Radiation Dose Estimate

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  | CONTAINS | CONTAINER | EV (128402, DCM, "Radiation Dose Estimate") | 1 | M |  |
2 | > | HAS CONCEPT MOD | TEXT | EV (128403, DCM, "Radiation Dose Estimate Name") | 1 | M |  |
3 | > | CONTAINS | TEXT | EV (121106, DCM, "Comment") | 1 | U |  |
4 | > | CONTAINS | INCLUDE | DTID 10033 “Radiation Dose Estimate Methodology” | 1 | M |  |
5 | > | CONTAINS | INCLUDE | DTID 10032 “Radiation Dose Estimate Representation” | 1-n | U |  |
6 | > | CONTAINS | CONTAINER | EV (113517, DCM, "Organ Radiation Dose Information") | 1-n | M |  |
7 | >> | CONTAINS | CODE | EV (113343008, SCT, "Organ") | 1 | M |  | DCID 10060 “Organs for Radiation Dose Estimates”
8 | >>> | HAS CONCEPT MOD | CODE | EV (272741003, SCT, "Laterality") | 1 | MC | IF Row 7 has laterality | DCID 244 Laterality
9 | >> | CONTAINS | TEXT | EV (121106, DCM, "Comment") | 1 | U |  |
10 | >> | CONTAINS | NUM | DCID 10061 “Absorbed Radiation Dose Types” | 1 | M |  | UNITS = EV (mGy, UCUM, "mGy")
11 | >>> | HAS PROPERTIES | NUM | DCID 225 “Measurement Uncertainty Concepts” | 1-n | U |  | UNITS = EV (mGy, UCUM, "mGy")
12 | >>>> | HAS PROPERTIES | TEXT | EV (128511, DCM, "Reference to Uncertainty Determination Method") | 1 | U |  |
13 | >> | CONTAINS | NUM | DCID 10062 “Equivalent Radiation Dose Types” | 1 | U |  | UNITS = EV (mSv, UCUM, "mSv")
14 | >>> | HAS PROPERTIES | NUM | DCID 225 “Measurement Uncertainty Concepts” | 1-n | U |  | UNITS = EV (mSv, UCUM, "mSv")
15 | >>>> | HAS PROPERTIES | TEXT | EV (128511, DCM, "Reference to Uncertainty Determination Method") | 1 | U |  |

Content Item Descriptions

Row 13 | Equivalent Dose is an international quantity and includes the use of a Radiation Weighting Factor to compensate for the radiation type, e.g., photon, neutron, alpha or beta particle, etc. Stating equivalent dose is not recommended in almost all dosimetry situations, except in Radiopharmaceutical dose. This is not Effective Dose.

Prev | Up | Next
Patient Radiation Dose SR IOD Templates | Home | TID 10032 Radiation Dose Estimate Representation

DICOM PS3.16 2020c - Content Mapping Resource