DICOM PS3.4 2020c - Service Class Specifications

H.4.5 Print Job SOP Class (Current)
Prev | H.4 Print Management SOP Class Definitions | Next

### H.4.5 Print Job SOP Class

#### H.4.5.1 IOD Description

The Print Job IOD is an abstraction of the Print Job transaction and is the basic information entity to monitor the execution of the Print Process. A Print Job contains one film or multiple films, all belonging to the same film session.

The Print Job SOP Class is created by N-ACTION operation of the Film Session SOP Class, Film Box SOP Class, or Pull Print Request SOP Class. The Print Job SOP Instance is deleted after the films are printed or after a failure condition.

Prev | Up | Next
H.4.4.3 SOP Class Definition and UID | Home | H.4.5.2 DIMSE Service Group

DICOM PS3.4 2020c - Service Class Specifications