DICOM PS3.18 2020c - Web Services

9.5.2.4 Source Image Region (Current)
Prev | 9.5.2 Behavior | Next

#### 9.5.2.4 Source Image Region

If this Query Parameter is supported and present:

- An image matrix corresponding to the region specified by Source Image Region shall be returned with its size corresponding to the specified normalized coordinate values.

- If the Presentation UID parameter is present, the region shall be selected after the corresponding presentation state has been applied on the images.

However, if any of the following are true:

- the Query Parameter specifies an ill-defined region,

- there are greater or fewer than four parameter values present, or

- any of the parameters do not conform to the requirements specified in Section 9.5.1.2.5

the origin server shall return a 400 (Bad Request) response and may include a payload containing an appropriate error message.

Prev | Up | Next
9.5.2.3 Presentation State | Home | 9.5.2.5 Viewport

DICOM PS3.18 2020c - Web Services