DICOM PS3.4 2020c - Service Class Specifications

DD.3.2.2.3 Status (Current)
Prev | DD.3.2.2 N-GET | Next

##### DD.3.2.2.3 Status

Table DD.3.2.2.3-1 defines the status code values that might be returned in a N-GET response. General status code values and fields related to status code values are defined for N-GET DIMSE Service in PS3.7.

Table DD.3.2.2.3-1. RT Conventional Machine and RT Ion Machine Verification SOP Class N-GET Status Values

Service Status | Further Meaning | Status Code
--- | --- | ---
Success | Treatment Verification Status of the applicable Machine Verification instance successfully returned. | 0000
Failure | Failed: Applicable Machine Verification instance not found | C112

Prev | Up | Next
DD.3.2.2.2 Attributes | Home | DD.3.2.2.4 Behavior

DICOM PS3.4 2020c - Service Class Specifications