DICOM PS3.2 2020d - Conformance

E.4.3.2 Additional Protocols (Current)
Prev | E.4.3 Network Interfaces | Next

### E.4.3.2 Additional Protocols

DHCP can be used to obtain TCP/IP network configuration information (e.g., own TCP/IP address, net-mask, default gateway, DNS server, etc). Support for DHCP can be configured via the Configuration Service/Installation Tool. . If DHCP is not in use, TCP/IP network configuration information can be manually configured via the Service/Installation Tool.

DNS can be used for address resolution. If DHCP is not in use, the identity of a DNS server can be configured via the Service/Installation Tool. If a DNS server is not in use, local mapping between hostname and TCP/IP address can be manually configured via the Service/Installation Tool.

Prev | Up | Next
E.4.3 Network Interfaces | Home | E.4.3.3 IPv4 and IPv6 Support

DICOM PS3.2 2020d - Conformance