DICOM PS3.6 2020d - Data Dictionary

7 Registry of DICOM File Meta Elements (Current)
Prev |  | Next

# 7 Registry of DICOM File Meta Elements

This section specifies the File Meta Elements needed to support the formatting of the File Meta Information of the DICOM File Format (see PS3.10).

Table 7-1. Registry of DICOM File Meta Elements

Tag | Name | Keyword | VR | VM |
--- | --- | --- | --- | --- | ---
(0002,0000) | File Meta Information Group Length | File​Meta​Information​Group​Length | UL | 1 |
(0002,0001) | File Meta Information Version | File​Meta​Information​Version | OB | 1 |
(0002,0002) | Media Storage SOP Class UID | Media​Storage​SOP​Class​UID | UI | 1 |
(0002,0003) | Media Storage SOP Instance UID | Media​Storage​SOP​Instance​UID | UI | 1 |
(0002,0010) | Transfer Syntax UID | Transfer​Syntax​UID | UI | 1 |
(0002,0012) | Implementation Class UID | Implementation​Class​UID | UI | 1 |
(0002,0013) | Implementation Version Name | Implementation​Version​Name | SH | 1 |
(0002,0016) | Source Application Entity Title | Source​Application​Entity​Title | AE | 1 |
(0002,0017) | Sending Application Entity Title | Sending​Application​Entity​Title | AE | 1 |
(0002,0018) | Receiving Application Entity Title | Receiving​Application​Entity​Title | AE | 1 |
(0002,0026) | Source Presentation Address | Source​Presentation​Address | UR | 1 |
(0002,0027) | Sending Presentation Address | Sending​Presentation​Address | UR | 1 |
(0002,0028) | Receiving Presentation Address | Receiving​Presentation​Address | UR | 1 |
(0002,0031) | RTV Meta Information Version | RTV​Meta​Information​Version | OB | 1 |
(0002,0032) | RTV Communication SOP Class UID | RTV​Communication​SOP​Class​UID | UI | 1 |
(0002,0033) | RTV Communication SOP Instance UID | RTV​Communication​SOP​Instance​UID | UI | 1 |
(0002,0035) | RTV Source Identifier | RTV​Source​Identifier | OB | 1 |
(0002,0036) | RTV Flow Identifier | RTV​Flow​Identifier | OB | 1 |
(0002,0037) | RTV Flow RTP Sampling Rate | RTV​Flow​RTP​Sampling​Rate | UL | 1 |
(0002,0038) | RTV Flow Actual Frame Duration | RTV​Flow​Actual​Frame​Duration | FD | 1 |
(0002,0100) | Private Information Creator UID | Private​Information​Creator​UID | UI | 1 |
(0002,0102) | Private Information | Private​Information | OB | 1 |

Prev |  | Next
6 Registry of DICOM Data Elements | Home | 8 Registry of DICOM Directory Structuring Elements

DICOM PS3.6 2020d - Data Dictionary