DICOM PS3.17 2020d - Explanatory Information

T.4 Quantitative Arterial Analysis Reference Method (Current)
Prev | T Quantitative Analysis References (Informative) | Next

## T.4 Quantitative Arterial Analysis Reference Method

Defined Terms:

- Computer Calculated Reference.

- Interpolated Local Reference.

- Mean Local Reference.

### T.4.1 Computer Calculated Reference

The computer-defined obstruction analysis calculates the reconstruction diameter based on the diameters outside the stenotic segment. This method is completely automated and user independent. The reconstructed diameter represents the diameters of the artery had the obstruction not been present.

The proximal and distal borders of the stenotic segment are automatically calculated.

The difference between the detected contour and the reconstructed contour inside the reconstructed diameter contour is considered to be the plaque.

Based on the reconstruction diameter at the Minimum Luminal Diameter (MLD) position a reference diameter for the obstruction is defined.

Prev | Up | Next
T.3.4 Radial Based Wall Motion Region | Home | T.4.2 Interpolated Reference

DICOM PS3.17 2020d - Explanatory Information