DICOM PS3.18 2020d - Web Services

12.5.3.2 Response Header Fields (Current)
Prev | 12.5.3 Response | Next

#### 12.5.3.2 Response Header Fields

Table 12.5.3-2. Response Header Fields

Header Field | Value | Origin Server Usage | Requirements
--- | --- | --- | ---
Content-Type | dicom-media-type | M | The media type of the response payload.
Content-Length | uint | C | Shall be present if a content encoding has not been applied to the payload
Content-Encoding | encoding | C | Shall be present if a content encoding has been applied to the payload

See also Section 8.4.

Prev | Up | Next
12.5.3 Response | Home | 12.5.3.3 Response Payload

DICOM PS3.18 2020d - Web Services