DICOM PS3.18 2020e - Web Services

10.6.3.2 Response Header Fields (Current)
Prev | 10.6.3 Response | Next

#### 10.6.3.2 Response Header Fields

The origin server shall support header fields as required in Table 10.6.3-2.

Table 10.6.3-2. Response Header Fields

Name | center | Origin Server Usage | Description
--- | --- | --- | ---
Content-Type | media-type | C | The DICOM Media Type of the response payload Shall be present if the response has a payload
Content-Length | uint | C | Shall be present if no content coding has been applied to the payload
Content-Encoding | encoding | C | Shall be present if a content encoding has been applied to the payload

Prev | Up | Next
10.6.3 Response | Home | 10.6.3.3 Response Payload

DICOM PS3.18 2020e - Web Services