DICOM PS3.3 2020e - Information Object Definitions

A.85.2.4 Encapsulated OBJ IOD Content Constraints (Current)
Prev | A.85.2 Encapsulated OBJ IOD | Next

#### A.85.2.4 Encapsulated OBJ IOD Content Constraints

##### A.85.2.4.1 Encapsulated Document

The Encapsulated Document (0042,0011) Attribute shall contain an ASCII OBJ byte stream [OBJ].

### Note

The Frame Of Reference UID (0020,0052) is an identifier for the origin and axes implicit in the OBJ data.

Prev | Up | Next
A.85.2.3 Encapsulated OBJ IOD Module Table | Home | A.85.2.4.2 MIME Type of Encapsulated Document

DICOM PS3.3 2020e - Information Object Definitions