DICOM PS3.18 2020e - Web Services

8.7.4 Rendered Media Types (Current)
Prev | 8.7 Media Types | Next

### 8.7.4 Rendered Media Types

DICOM Instances may be converted by a rendering process into non-DICOM Media Types. This can be useful to display or process them using non-DICOM software, such as browsers.

For example, an Instance containing:

1. an image could be rendered into the image/jpeg or image/png Rendered Media Types.

2. a multi-frame image in a lossless Transfer Syntax could be rendered into a video/mpeg or video/mp4 Rendered Media Type.

3. a Structured Report could be rendered into a text/html, text/plain, or application/pdf Rendered Media Type.

### Note

Rendered Media Types are usually consumer format media types. Some of the same non-DICOM Media Types are also used as Bulkdata Media Types, that is, for encoding Bulkdata extracted from Encapsulated Pixel Data (used with compressed Transfer Syntaxes), without applying a rendering process. See Section 8.7.3.3.

Rendered images shall contain no more than 8 bits per channel.

Origin servers shall support rendering Instances of different Resource Categories into Rendered Media Types as specified in Table 8.7.4-1.

Table 8.7.4-1. Rendered Media Types by Resource Category

Category | Media Type | URI | RESTful
--- | --- | --- | ---
Single Frame Image | image/jpeg | D | D
image/gif | O | R
image/png | O | R
image/jp2 | O | O
Multi-frame Image | image/gif | O | O
Video | video/mpeg | O | O
video/mp4 | O | O
video/H265 | O | O
Text | text/html | D | D
text/plain | R | R
text/xml | O | R
text/rtf | O | O
application/pdf | O | O

When an image/jpeg media type is returned, the image shall be encoded using the JPEG baseline lossy 8-bit Huffman encoded non-hierarchical non-sequential process defined in [ISO/IEC 10918-1].

The origin server may support additional Rendered Media Types, which shall be documented in the Conformance Statement and, if the service supports it, the Retrieve Capabilities response.

A Transfer Syntax media type parameter is not permitted for Rendered Media Types.

Prev | Up | Next
8.7.3.7 Acceptable Transfer Syntaxes | Home | 8.7.5 Acceptable Media Types

DICOM PS3.18 2020e - Web Services