DICOM PS3.17 2020e - Explanatory Information

XXX.4.2 Structured Displays (Current)
Prev | XXX.4 Uses of Presentation View Description in the Identification Module | Next

### XXX.4.2 Structured Displays

A Structured Display Instance could select a set of one or more Volumetric Presentation States by defining an image box whose Image Box Layout Type (0072,0304) has a Value of "VOLUME_VIEW" or "VOLUME_CINE" and by specifying one or more Volumetric Presentation States using the Referenced Presentation State Sequence (see Table C.11.17-1 “Structured Display Image Box Module Attributes” in PS3.3).

Prev | Up | Next
XXX.4 Uses of Presentation View Description in the Identification Module | Home | XXX.4.3 Ad Hoc Display Layout

DICOM PS3.17 2020e - Explanatory Information