DICOM PS3.16 2020e - Content Mapping Resource

TID 10034 Radiation Dose Estimate Parameters (Current)
Prev | Patient Radiation Dose SR IOD Templates | Next

### TID 10034 Radiation Dose Estimate Parameters

This template includes the parameters that are specific to the Radiation Dose Estimate Method used in the algorithms when estimating dose to individual organs, phantoms, or the entire body from imaging studies that use ionizing radiation.

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 10034. Radiation Dose Estimate Parameters

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (128434, DCM, "Radiation Dose Estimate Parameters") | 1 | M |  |
2 | > | CONTAINS | NUM | DCID 10069 “Radiation Dose Estimation Parameter ” | 1-n | MC | IF Row 4 absent | UNITS = DCID 82 “Units of Measurement”
4 | > | CONTAINS | COMPOSITE | EV (128436, DCM, "Radiation Dose Composite Parameters") | 1-n | MC | IF Row 2 absent |
5 | >> | CONTAINS | TEXT | EV (121106, DCM, "Comment") | 1 | U |  |

Content Item Descriptions

Row 2 | These are the parameters of the method specified in Row 43 of TID 10033 “Radiation Dose Estimate Methodology”. The code meanings should correlate directly with the names of the parameters used in the methodology documentation.
Row 4 | References to Parametric Map Image, Mesh, encapsulated pdf, or other similar IOD.
Row 5 | Describes the contents of the IOD referenced in Row 4

Prev | Up | Next
TID 10033 Radiation Dose Estimate Methodology | Home | Imaging Agent Administration SR IOD Templates

DICOM PS3.16 2020e - Content Mapping Resource